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SECTION 34 41 00
CAR1806 Vehicle Exiting Alley Warning Sign Systems
Construction A&E Master Specification
	Primary classification
	CSI MasterFormat 34 41 00 Roadway Signaling and Control Equipment

	Basis of design
	Pass Signs CAR1806 Vehicle Exiting Alley Warning Sign Systems

	Manufacturer
	Parking Alert Signs, Phoenix, Arizona

	Product families
	CAR1806V3, CAR1806V3-DL, and CAR1806V3-DL-Dual

	Issue
	Master specification for project editing

	Revision date
	September 30, 2026


Purpose and use  This section specifies a complete intelligent vehicle-exit warning system for alleys, compact parking exits, blind driveways, and tight drive lanes. The design professional should edit project choices, coordinate final mounting and detection locations with the drawings, and confirm applicable codes and authority requirements before issue for construction.
Classification guidance  Use Section 34 41 00 as the primary location because the equipment detects traffic or pedestrian activity and controls active visual warnings. Coordinate static sign requirements with Section 10 14 00 Signage and branch power, raceways, grounding, and field wiring with Division 26 Electrical.
PART 1 GENERAL
1.1 SUMMARY
A. Section includes intelligent vehicle-exit warning system with CAR and VEHICLE EXITING warning output, programmable controller, power supply, and project-selected or furnished triggering equipment.
B. Provide a complete, coordinated, and operational system. Furnish components, internal wiring, factory programming, mounting provisions, labels, and installation documentation required for the selected configuration.
C. Related requirements include Section 10 14 00 Signage, Division 26 Electrical, and Division 28 Electronic Safety and Security where interfaces to gates, doors, access control, or security equipment are required.
1.2 REFERENCES
A. Comply with current adopted editions of CSI MasterFormat Section 34 41 00, NFPA 70, applicable state and local requirements, and manufacturer installation, wiring, mounting, and programming instructions.
1.3 SYSTEM DESCRIPTION
A. The system shall receive a vehicle trigger, flash the illuminated warning text, and play the programmed vehicle-exit announcement.
B. The controller shall maintain the active state for the programmed interval. A valid new trigger during an active cycle shall restart or extend the timer as required by the approved operating sequence.
C. Final timing, sign orientation, detector placement, sensitivity, and output behavior shall be established during commissioning and approved by the Owner.
D. Provide adjustable audible output and a programmable quiet-hour schedule that suppresses audio while visual warnings remain active.
1.4 ACTION SUBMITTALS
A. Product data for sign or signal assemblies, controller, power supply, furnished sensors, mounting hardware, and accessories.
B. Shop drawings showing locations, heights, orientations, viewing directions, detection zones, controller location, raceways, conductors, and service clearances.
C. Point-to-point wiring diagrams identifying branch power, 12 VDC power, inputs, outputs, interfaces, and terminal designations.
D. Programming schedule stating timing, output sequence, detection logic, and final project settings.
E. Product schedule identifying the selected model and configuration at each location.
1.5 INFORMATIONAL SUBMITTALS
A. Installer qualifications and experience with comparable low-voltage warning, detection, or traffic-control systems.
B. Manufacturer warranty documentation and field-test report identifying final settings, results, and corrective action.
1.6 CLOSEOUT SUBMITTALS
A. Operation and maintenance manuals, installation and programming instructions, wiring diagrams, troubleshooting information, record drawings, and the final commissioning record.
1.7 QUALITY ASSURANCE
A. Provide signs or signals, controller, power supply, and furnished sensors as a coordinated system by one manufacturer.
B. Use installers experienced with low-voltage warning, traffic-control, parking-control, or comparable detection systems. Electrical work shall be performed by properly qualified personnel.
1.8 DELIVERY STORAGE AND HANDLING
A. Deliver equipment in manufacturer packaging. Store in a clean, dry, secure location and protect finishes, lenses, electronics, sensors, and terminals from damage.
1.9 WARRANTY
A. Provide manufacturer standard written warranty covering defects in materials and workmanship. Submit terms with product data.


PART 2 PRODUCTS
2.1 MANUFACTURER
A. Basis of Design: Parking Alert Signs, Pass Signs brand, Phoenix, Arizona; telephone 480-689-1993; email Support@PassSigns.com; website https://passsigns.com.
B. Substitutions shall comply with Division 01 and meet every functional, dimensional, environmental, material, control, documentation, and commissioning requirement in this section.
2.2 PRODUCT CONFIGURATIONS
Provide the configuration scheduled on the drawings and listed below.
	Model
	Configuration
	Major equipment included
	Trigger arrangement

	CAR1806V3
	Sign system
	One CAR1806 sign; PSC-5 controller; PS126A power supply
	Project-furnished compatible dry-contact trigger or gate/door interface

	CAR1806V3-DL
	Single-lane kit
	One CAR1806 sign; PSC-5 controller; PS126A power supply; one Decider2 detector
	Directional detection for one exit lane

	CAR1806V3-DL-Dual
	Wide-exit dual-sign kit
	Two CAR1806 signs; PSC-5 controller; PS126A power supply; one Decider2 detector
	One exit lane with warnings visible across a wide opening



2.3 PERFORMANCE REQUIREMENTS
A. System shall be factory-coordinated for the selected configuration and furnished ready for mounting, power connection, trigger connection, programming verification, and commissioning.
B. A valid operating command shall activate the required CAR and VEHICLE EXITING warning output for the programmed operating interval.
C. Controller shall restart or extend the active interval when an additional valid trigger is received, unless the approved sequence specifically requires queuing or priority logic.
D. Equipment exposed to the environment shall be suitable for direct outdoor exposure. Field boxes, raceways, fittings, and seals shall suit the installed environment.
2.4 WARNING OR SIGNAL ASSEMBLY
A. Warning output: High-visibility CAR and VEHICLE EXITING display arranged for clear viewing from the intended approaches.
B. Dimensions: Nominal 18 inches high by 6 inches wide by 8 inches deep, with three-sided text.
C. Construction: 14-gauge aluminum, with manufacturer standard powder-coated hammered-copper finish.
D. Arrange enclosures and components for service access without removing permanent building construction. Provide corrosion-resistant mounting hardware suited to the substrate and exposure.
2.5 CONTROLLER
A. Controller: Pass Signs PSC-5 Intelligent Sign Controller furnished as part of the complete system.
B. Controller shall accept the specified trigger inputs, command required outputs, control timing, implement the approved sequence, and identify terminals to match submitted wiring diagrams.
2.6 POWER SUPPLY
A. Power supply: Pass Signs PS126A, 100-240 VAC input and 12 VDC output, coordinated with the selected controller, warning equipment, sensors, and configuration.
B. Provide branch-circuit connection, disconnecting means, overcurrent protection, grounding, raceways, and field wiring under Division 26.
2.7 AUDIBLE WARNING
A. Provide manufacturer-coordinated speaker and programmed warning message for each required sign assembly.
B. Provide adjustable level and scheduled audio cut-off. Set final volume for intelligibility in the warning area without unnecessary disturbance in adjacent occupied areas.
2.8 TRIGGER DEVICES AND INTERFACES
A. Trigger equipment: Decider2 intelligent vehicle motion detector.
B. Locate and adjust detection equipment to recognize intended activity while limiting nuisance activation from cross traffic, pedestrians, doors, fans, vibration, reflective surfaces, or unrelated movement.
C. Provide mounting hardware, wiring accessories, interfaces, and labels required for the selected installation.
2.9 FACTORY PREPARATION
A. Assemble and prewire components to the maximum extent practical. Program standard operating logic before shipment and verify final project settings during commissioning.
B. Provide durable identification for equipment, terminals, conductors, and field connection points.


PART 3 EXECUTION
3.1 EXAMINATION
A. Verify that mounting substrates are complete, secure, and capable of supporting equipment loads.
B. Verify branch power, pathways, field wiring, interfaces, drainage, sight lines, detection coverage, and service clearances. Do not begin until unsatisfactory conditions are corrected.
3.2 INSTALLATION
A. Install equipment in accordance with approved submittals, manufacturer instructions, Contract Documents, and applicable codes.
B. Mount assemblies plumb, level, rigid, and oriented for clear viewing. Maintain service access and required clearances.
C. Install power and control wiring in approved raceways, separate circuits as required, protect conductors from damage and moisture, and label both ends.
D. Seal exterior penetrations and entries. Provide appropriate anchors, corrosion-resistant fasteners, drip loops, and drainage provisions.
E. Mount and adjust detectors at approved locations. Coordinate interfaces to gates, doors, loops, access control, and project-furnished triggers before energizing.
3.3 PROGRAMMING
A. Program activation duration, output sequence, priority or queue logic, detector settings, and other approved project parameters.
B. Record final settings in the operation and maintenance manuals and commissioning report.
3.4 FIELD QUALITY CONTROL
A. Inspect secure mounting, orientation, weather sealing, conductor identification, grounding, and service access.
B. Test and document activation from each intended source, rejection of unrelated activity, correct warning output at every required approach, timer behavior, recovery after power interruption, and operation of every furnished configuration.
C. Verify audible message clarity, acceptable volume, quiet-hour cut-off, and continued visual warning during audio suppression.
D. Correct deficiencies and repeat testing until the system operates as specified.
3.5 COMMISSIONING
A. Commission with the Owner representative present. Observe representative traffic or pedestrian activity and adjust placement, aim, sensitivity, timing, and sequence for reliable operation.
B. Submit the completed commissioning report and final programming record.
3.6 DEMONSTRATION AND TRAINING
A. Demonstrate normal operation, testing, programming, troubleshooting, and routine maintenance to Owner personnel.
3.7 CLEANING AND PROTECTION
A. Remove protective films and construction residue. Protect installed equipment until Substantial Completion and replace damaged components.
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